Cmp-Mod V01 Created by CvPcb (2012-12-10 BZR 3841)-testing date = Mon 10 Dec 2012 08:32:48 PM CET

BeginCmp
TimeStamp = /50C62534;
Reference = D1;
ValeurCmp = LED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /50C6254D;
Reference = D2;
ValeurCmp = LED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /50C6255C;
Reference = D3;
ValeurCmp = LED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /50C6256B;
Reference = D4;
ValeurCmp = LED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /50C6257A;
Reference = D5;
ValeurCmp = LED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /50C62589;
Reference = D6;
ValeurCmp = LED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /50C625A2;
Reference = D7;
ValeurCmp = LED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /50C625B1;
Reference = D8;
ValeurCmp = LED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /50C63640;
Reference = D9;
ValeurCmp = LED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /50C63664;
Reference = D10;
ValeurCmp = LED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /50C63646;
Reference = D11;
ValeurCmp = LED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /50C6364C;
Reference = D12;
ValeurCmp = LED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /50C63652;
Reference = D13;
ValeurCmp = LED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /50C63658;
Reference = D14;
ValeurCmp = LED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /50C6365E;
Reference = D15;
ValeurCmp = LED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /50C6366A;
Reference = D16;
ValeurCmp = LED;
IdModule  = LED-0805;
EndCmp

BeginCmp
TimeStamp = /50C62311;
Reference = P1;
ValeurCmp = CONN_9;
IdModule  = SIL-9;
EndCmp

BeginCmp
TimeStamp = /50C62340;
Reference = R1;
ValeurCmp = 1k;
IdModule  = -R0603;
EndCmp

BeginCmp
TimeStamp = /50C62356;
Reference = R2;
ValeurCmp = 1k;
IdModule  = -R0603;
EndCmp

BeginCmp
TimeStamp = /50C62379;
Reference = R3;
ValeurCmp = 1k;
IdModule  = -R0603;
EndCmp

BeginCmp
TimeStamp = /50C62388;
Reference = R4;
ValeurCmp = 1k;
IdModule  = -R0603;
EndCmp

BeginCmp
TimeStamp = /50C623E7;
Reference = R5;
ValeurCmp = 1k;
IdModule  = -R0603;
EndCmp

BeginCmp
TimeStamp = /50C623F6;
Reference = R6;
ValeurCmp = 1k;
IdModule  = -R0603;
EndCmp

BeginCmp
TimeStamp = /50C62405;
Reference = R7;
ValeurCmp = 1k;
IdModule  = -R0603;
EndCmp

BeginCmp
TimeStamp = /50C62414;
Reference = R8;
ValeurCmp = 1k;
IdModule  = -R0603;
EndCmp

EndListe
